{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":129,"n_cols":6,"rows_kept":129,"flags":["formulas_cached_only"]}
["序号","物料名称","规格型号","单位","数量","备注"]
[1,"AGC微量氧补充液","规格：M110672-2；品牌：北京凯隆","瓶",4]
[2,"AGC微量氧电解液","规格：M110672-1；品牌：北京凯隆","瓶",1]
[3,"磷表标液","品牌：Emerson  型号：phosphate standard；P/N 190-B0-021-01;浓度1000mg/L;50mL装","瓶",1]
[4,"硅表标液","品牌：Emerson  型号：silice standard；P/N 190-B0-021-01;浓度10ug/mL；50mL装","瓶",1]
[5,"标气","H2:1.97×10-2，平衡气Air，充装压力9.5MPa，钢瓶体积4L","瓶",1]
[6,"标气","i-C4H10:0.898%，平衡气Air，充装压力9.5MPa，钢瓶体积4L","瓶",1]
[7,"标气","O2:14.8%，平衡气N2，充装压力9.5MPa，钢瓶体积4L","瓶",1]
[8,"标气","CO:51ppm，平衡气N2，充装压力9.5MPa，钢瓶体积4L","瓶",1]
[9,"标气","氨气：50.4×10-6，平衡气N2，充装压力9.5MPa，钢瓶体积4L","瓶",1]
[10,"ORP标液","国产ORP两点标液（ 86mV ），瓶装500ml","瓶",1]
[11,"ORP标液","国产ORP两点标液（256mV ），瓶装500ml","瓶",1]
[12,"电导率标液","电导率标液浓度1408us/cm，瓶装500ml","瓶",2]
[13,"电导率标液","电导率标液浓度12.85ms/cm，瓶装500ml","瓶",2]
[14,"电导率标液","电导率标液浓度100us/cm，瓶装500ml","瓶",2]
[15,"浊度标液","浊度标液浓度1500NTU，瓶装500ml","瓶",1]
[16,"浊度标液","浊度标液浓度100NTU，瓶装500ml","瓶",1]
[17,"硅表试剂","硅表试剂组：190-B0-011（成品液体），品牌：艾默生","套",2]
[18,"磷表试剂","磷表试剂组：190-P0-011（成品液体），品牌：艾默生","套",2]
[19,"COD试剂","COD试剂组：REAG-COD，品牌：艾默生","套",2]
[20,"氨氮试剂","氨氮试剂组：REAG-AM ，品牌：艾默生","套",2]
[21,"余氯校准液","浓度5mg/L；100mL装","瓶",1]
[22,"标气","品牌：大特；充装压力：10MP;体积：8L；\n组分：二氧化碳4.9ppm，氮气（平衡）","瓶",1]
[23,"标气","品牌：大特；充装压力：10MP;体积：8L；\n组分：氧气（98-98.4%），氮气（平衡）","瓶",1]
[24,"标气","品牌：大特；充装压力：10MP;体积：8L；\n组分：氧气（8%），氮气（平衡）","瓶",1]
[25,"标气","品牌：大特；充装压力：10MP;体积：8L；\n组分：氧气（50%），氮气（平衡）","瓶",1]
[26,"标气","品牌：大特；充装压力：10MP;体积：8L；\n组分：氧气（4.5%），氮气（平衡）","瓶",1]
[27,"标气","品牌：大特；充装压力：10MP;体积：8L；\n组分：氧气（7.92%），氮气（平衡）","瓶",1]
[28,"标气","品牌：大特；充装压力：10MP;体积：8L；\n组分：二氧化碳（1600ppm），氮气（平衡）","瓶",1]
[29,"标气","品牌：大特；充装压力：10MP;体积：8L；\n组分：氩气（14-15%），氧气（平衡）","瓶",1]
[30,"标气","品牌：大特；充装压力：10MP;体积：8L；\n组分：一氧化二氮（80ppm），氮气（平衡）","瓶",1]
[31,"标气","品牌：大特；充装压力：10MP;体积：8L；\n组分：氩气（80-81%），氮气（平衡）","瓶",1]
[32,"标气","品牌：大特；充装压力：10MP;体积：8L；\n组分：氧气（18ppm），氮气（平衡）","瓶",1]
[33,"标气","品牌：大特；充装压力：10MP;体积：8L；\n组分：氧气（8ppm），氩气（平衡）","瓶",1]
[34,"标气","品牌：大特；充装压力：10MP;体积：8L；\n组分：N2 99.999%","瓶",6]
[35,"标气","品牌：大特；充装压力：10MP;体积：8L；\n组分：CO 1%- 余N2","瓶",2]
[36,"标气","品牌：大特；充装压力：10MP;体积：8L；\n组分：02 2.5%-余N2","瓶",1]
[37,"标气","品牌：大特；充装压力：10MP;体积：8L；\n组分：02 24%-余N2","瓶",2]
[38,"标气","品牌：大特；充装压力：10MP;体积：8L；\n组分：CH4 1994ppm-余N2","瓶",1]
[39,"标气","品牌：大特；充装压力：10MP;体积：8L；\n组分：二氧化碳（9.5-10ppm），氮气（平衡）","瓶",1]
[40,"标气","品牌：大特；充装压力：10MP;体积：8L；\n组分：一氧化碳（9.5-10ppm），氮气（平衡）","瓶",1]
[41,"标气","品牌：大特；充装压力：10MP;体积：8L；\n组分：氢气（80%），氮气（平衡）","瓶",1]
[42,"标气","品牌：大特；充装压力：10MP;体积：8L；\n组分：一氧化碳（10%），氮气（平衡）","瓶",1]
[43,"标气","品牌：大特；充装压力：10MP;体积：8L；\n组分：一氧化碳（3%），氮气（平衡）","瓶",1]
[44,"标气","品牌：大特；充装压力：10MP;体积：8L；\n组分：硫化氢（2%），氮气平衡","瓶",1]
[45,"标气","品牌：大特；充装压力：10MP;体积：8L；\n组分：二氧化硫1%，氮气平衡","瓶",1]
[46,"标气","品牌：大特；充装压力：10MP;体积：8L；\n组分：氧气1%，氮气平衡","瓶",3]
[47,"标气","品牌：大特；充装压力：10MP;体积：8L；\n组分：氧气18.14%，氮气平衡","瓶",3]
[48,"标气","品牌：大特；充装压力：10MP;体积：8L；\n组分：氢气89.87*10-2，氮气平衡","瓶",1]
[49,"标气","品牌：大特；充装压力：10MP;体积：8L；\n组分：一氧化碳7.98*10-6，氮气平衡","瓶",1]
[50,"余氯电解液","厂家：E+H;型号：CCV05余氯电解液1瓶， 50 ml (1.69 f1.0z)电解液","瓶",1]
[51,"溶解氧分析仪电解液","厂家：Emerson 型号：EMR56-92103671-A12","瓶",2]
[52,"溶解氧分析仪膜片","厂家：Emerson 型号：EMR56-23400562-M32","个",2]
[53,"电动执行器","厂家：天津中仪自动化仪表有限公司\n型号：ZY-RFZ1840/F1220","台",1]
[54,"电动执行器","厂家：天津中仪自动化仪表有限公司\n型号：ZY-RFZ18160/F1240","台",1]
[55,"跳线","光纤跳线SC-LC(UPC) 5米 单模双工尾纤（9/125 2.0）\n阻燃低烟无卤跳纤光纤线 型号：BY-5512S","根",4]
[56,"安全栅","厂家：北京平和创业科技发展有限公司\n型号：PHD-22TD-2121","个",4]
[57,"安全栅","型号：NPEXA-C5D111厂家：南京优倍电气","个",4]
[58,"安全栅","型号：NPEXA-C511  厂家：南京优倍电气","个",4]
[59,"安全栅","型号：NPEXA-CM31厂家：南京优倍电气","个",4]
[60,"调速阀","AS3201FG-03-12S","个",10]
[61,"上切刀",106053,"个",3]
[62,"下切刀",106083,"个",3]
[63,"钩针","033121","个",3]
[64,"交流接触器","LC1-D09M7C","个",1]
[65,"交流接触器","LC1-D09BL","个",1]
[66,"断路器辅助触点","GV-AN11","个",2]
[67,"滚子链活节","10A","个",5]
[68,"快速接头","KQ2VT12-04NS","个",5]
[69,"快速接头","NPQP-T-Q12-Q10-FD-P10","个",5]
[70,"快速接头","NPQP-Y-Q12-Q10-FD-P10","个",5]
[71,"快速接头","NPQP-L-R38-Q12-FD-P10","个",5]
[72,"快速接头","NPQP-L-R38-Q10-FD-P10","个",5]
[73,"快速接头","NPQP-D-R14-Q10-FD-P10","个",5]
[74,"快速接头","NPQP-D-Q12-Q10-FD-P10","个",5]
[75,"快速接头","NPQP-L-R14-Q10-FD-P10","个",5]
[76,"快速接头","KGL08-02","个",5]
[77,"快速接头","KGL08-01","个",5]
[78,"快速接头","KGW08-02","个",5]
[79,"快速接头","KGL10-02S","个",5]
[80,"快速接头","KGW10-02","个",5]
[81,"快速接头","NPQP-T-Q8-E-FD-P10","个",5]
[82,"快速接头","NPQP-L-R14-Q8-FD-P10","个",5]
[83,"快速接头","NPQP-L-R18-Q8-FD-P10","个",5]
[84,"快速接头","NPQP-L-R18-Q6-FD-P10","个",5]
[85,"快速接头","KFG2H0806-01","个",5]
[86,"快速接头","NPQP-Y-Q8-E-FD-P10","个",5]
[87,"快速接头","NPQP-T-Q8-Q6-FD-P10","个",5]
[88,"快速接头","NPQP-Y-Q8-Q6-FD-P10","个",5]
[89,"快速接头","NPQP-D-Q12-Q10-FD-P10","个",5]
[90,"快速接头","NPQP-D-Q10-Q8-FD-P10","个",5]
[91,"快速接头","KQ2R08-10A","个",5]
[92,"快速接头","KGH06-M5","个",5]
[93,"快速接头","NPQP-L-R18-Q8-FD-P10","个",5]
[94,"快速接头","KGL12-03","个",5]
[95,"快速接头","KGW12-03","个",5]
[96,"调速阀","AS3201FG-03-10S","个",5]
[97,"调速阀","AS2201FG-02-10S","个",5]
[98,"调速阀","AS2201FG-01-08S","个",5]
[99,"调速阀","AS2201FG-01-06S","个",5]
[100,"调速阀","AS3001FG-10","个",5]
[101,"气源三联件","AC60X-DNX5206","个",1]
[102,"固体润滑膏（耦合剂）","厂家：摩力克;型号：111 Compound,100g","瓶",1]
[103,"横河变送器EJA-E防雨罩","厂家：宁波江东苏甬机电有限公司;型号：200*125*90","个",10]
[104,"霍尼韦尔变送器ST700防雨罩","厂家：宁波江东苏甬机电有限公司;型号：196*151*86","个",30]
[105,"雷达液位计","位号：180-LT-1026，详见数据表","台",1]
[106,"检测式隔离安全栅","厂家：北京平和创业科技发展有限公司;型号：PH-22DF-2727 ","个",4]
[107,"输入隔离安全栅","厂家：北京平和创业科技发展有限公司;型号：PHD-22TF-2828 ","个",4]
[108,"PH探头","厂家：E+H;型号：CPS77E-NA6BBU2","个",1]
[109,"PH探头","厂家：E+H;型号：CPS11E-1035/0，CPS11E-BA7AAA2","个",1]
[110,"余氯探头","厂家：E+H;型号：CCV05，CCS51D-AA11AD+NB","个",1]
[111,"余氯覆膜帽","厂家：E+H;型号：CCV05余氯覆膜帽","个",2]
[112,"光模块","品牌：华为，1310","个",5]
[113,"24口六类RJ45配线架","品牌：爱普华顿AP-6-04-24X","套",2]
[114,"4芯单模光缆终端盒","品牌：大华，含尾纤","个",2]
[115,"发卡器","品牌：大华，H-ASM100，IC卡","个",2]
[116,"单模光纤跳线","接头：LC-LC,3m","个",10]
[117,"单模光纤跳线","接头：SC-LC,3m","个",10]
[118,"单模光纤跳线","接头：SC-SC,3m","个",10]
[119,"六类信息插（RJ45）","品牌：一舟，壁嵌式，带面板","个",10]
[120,"工业级光纤收发器","品牌：艾威世纪，J-1B","套",2]
[121,"尾纤","12芯圆头束状尾纤","个",10]
[122,"尾纤","12芯方头束状尾纤","个",10]
[123,"光纤热缩管","25mm微型裸纤熔接管","袋",5]
[124,"光纤适配器","FC-FC","个",20]
[125,"光纤适配器","SC-FC","个",20]
[126,"网线连接器","RJ-45","个",5]
[127,"交换机","品牌：华为，8口","个",4]
[128,"光功率计","30mW","个",2]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}